Failed to get ControllerId List.
Failed to get CpController object.

Exit Code: 0x01
Failed to get ControllerId List.
Failed to get CpController object.

Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00
Adapter 0: Get BBU Modes Failed.

FW error description: 
 The requested command is invalid.  

Exit Code: 0x02
Adapter 0: BBU MFG Sleep Succeeded.

Exit Code: 0x00
Adapter 0: BBU MFG Sleep Failed

Exit Code: 0x01
Adapter 0: BBU MFG SEAL Failed

Exit Code: 0x01
Adapter 0: Get BBU Status Failed.

Exit Code: 0x01
Adapter 0: Get BBU Status Failed.
Adapter 0: Get BBU ChargeTime Failed.
Adapter 0: Get BBU Capacity Info Failed.
Adapter 0: Get BBU Status Info Failed.
Adapter 0: Get BBU Properties Failed.

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4080 mV
Current: 68 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 97 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 92 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4080 mV
Current: 68 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 97 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 92 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4084 mV
Current: 53 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 98 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 92 %
Max Error: 2 %

Exit Code: 0x00

BBU Capacity Info for Adapter: 0

Relative State of Charge: 98 %
Absolute State of charge: 92 %
Remaining Capacity: 1122 mAh
Full Charge Capacity: 1147 mAh
Run time to empty: Battery is not being discharged 
Average time to empty: Battery is not being discharged 
Average Time to full: 30 min 
Cycle Count: 19
Max Error = 2 %
Remaining Capacity Alarm = 120 mAh
Remining Time Alarm = 10 Min

Exit Code: 0x00

BBU Design Info for Adapter: 0

Date of Manufacture: 11/24, 2009
Design Capacity: 1215 mAh
Design Voltage: 3700 mV
Specification Info: 33
Serial Number: 1110
Pack Stat Configuration: 0x64a0
Manufacture Name: LS1121001A
Device Name: 3150301
Device Chemistry: LION
Battery FRU: N/A

Transparent Learn = 0
App Data = 0

Exit Code: 0x00
Adapter 0: Get BBU Modes Failed.

FW error description: 
 The requested command is invalid.  

Exit Code: 0x02
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4086 mV
Current: 49 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 98 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 92 %
Max Error: 2 %

Battery backup charge time : 48 hours +

BBU Capacity Info for Adapter: 0

Relative State of Charge: 98 %
Absolute State of charge: 93 %
Remaining Capacity: 1124 mAh
Full Charge Capacity: 1147 mAh
Run time to empty: Battery is not being discharged 
Average time to empty: Battery is not being discharged 
Average Time to full: 28 min 
Cycle Count: 19
Max Error = 2 %
Remaining Capacity Alarm = 120 mAh
Remining Time Alarm = 10 Min

BBU Design Info for Adapter: 0

Date of Manufacture: 11/24, 2009
Design Capacity: 1215 mAh
Design Voltage: 3700 mV
Specification Info: 33
Serial Number: 1110
Pack Stat Configuration: 0x64a0
Manufacture Name: LS1121001A
Device Name: 3150301
Device Chemistry: LION
Battery FRU: N/A

Transparent Learn = 0
App Data = 0

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4086 mV
Current: 49 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 98 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 92 %
Max Error: 2 %

Battery backup charge time : 48 hours +

BBU Capacity Info for Adapter: 0

Relative State of Charge: 98 %
Absolute State of charge: 93 %
Remaining Capacity: 1124 mAh
Full Charge Capacity: 1147 mAh
Run time to empty: Battery is not being discharged 
Average time to empty: Battery is not being discharged 
Average Time to full: 28 min 
Cycle Count: 19
Max Error = 2 %
Remaining Capacity Alarm = 120 mAh
Remining Time Alarm = 10 Min

BBU Design Info for Adapter: 0

Date of Manufacture: 11/24, 2009
Design Capacity: 1215 mAh
Design Voltage: 3700 mV
Specification Info: 33
Serial Number: 1110
Pack Stat Configuration: 0x64a0
Manufacture Name: LS1121001A
Device Name: 3150301
Device Chemistry: LION
Battery FRU: N/A

Transparent Learn = 0
App Data = 0

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4087 mV
Current: 48 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 98 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 93 %
Max Error: 2 %

Battery backup charge time : 48 hours +

BBU Capacity Info for Adapter: 0

Relative State of Charge: 98 %
Absolute State of charge: 93 %
Remaining Capacity: 1125 mAh
Full Charge Capacity: 1147 mAh
Run time to empty: Battery is not being discharged 
Average time to empty: Battery is not being discharged 
Average Time to full: 27 min 
Cycle Count: 19
Max Error = 2 %
Remaining Capacity Alarm = 120 mAh
Remining Time Alarm = 10 Min

BBU Design Info for Adapter: 0

Date of Manufacture: 11/24, 2009
Design Capacity: 1215 mAh
Design Voltage: 3700 mV
Specification Info: 33
Serial Number: 1110
Pack Stat Configuration: 0x64a0
Manufacture Name: LS1121001A
Device Name: 3150301
Device Chemistry: LION
Battery FRU: N/A

Transparent Learn = 0
App Data = 0

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4086 mV
Current: 46 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Charging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : No
  Discharging             : No
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 98 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 512 mA
Absolute state of charge: 93 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4072 mV
Current: 0 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 94 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4071 mV
Current: 0 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : Yes
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 94 %
Max Error: 2 %

Exit Code: 0x00
Adapter 0: BBU Learn Succeeded.

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4069 mV
Current: 0 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : Yes
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : No
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 94 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4069 mV
Current: 0 mA
Temperature: 29 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : Yes
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : No
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 94 %
Max Error: 2 %

Exit Code: 0x00

BBU Properties for Adapter: 0

Auto Learn Period: 2592000 Sec
Next Learn time: 380712875 Sec 
Learn Delay Interval:0 Hours
Auto-Learn Mode: Disabled

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 3942 mV
Current: -461 mA
Temperature: 30 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : Discharging
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : Yes
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : No
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 99 %
Charger System State: 49169
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 94 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4060 mV
Current: 0 mA
Temperature: 26 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : No
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 88 %
Max Error: 2 %

Exit Code: 0x00
BBU status for Adapter: 0

BatteryType: iBBU
Voltage: 4060 mV
Current: 0 mA
Temperature: 26 C

Battery State     : Operational

BBU Firmware Status:

  Charging Status              : None
  Voltage                                 : OK
  Temperature                             : OK
  Learn Cycle Requested	                  : No
  Learn Cycle Active                      : No
  Learn Cycle Status                      : OK
  Learn Cycle Timeout                     : No
  I2c Errors Detected                     : No
  Battery Pack Missing                    : No
  Battery Replacement required            : No
  Remaining Capacity Low                  : No
  Periodic Learn Required                 : No
  Transparent Learn                       : No
  No space to cache offload               : No
  Pack is about to fail & should be replaced : No
  Cache Offload premium feature required  : No
  Module microcode update required        : No



GasGuageStatus:
  Fully Discharged        : No
  Fully Charged           : Yes
  Discharging             : Yes
  Initialized             : Yes
  Remaining Time Alarm    : No
  Remaining Capacity Alarm: No
  Discharge Terminated    : No
  Over Temperature        : No
  Charging Terminated     : No
  Over Charged            : No

Relative State of Charge: 100 %
Charger System State: 49168
Charger System Ctrl: 0
Charging current: 0 mA
Absolute state of charge: 88 %
Max Error: 2 %

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : LSI MegaRAID SAS 9260-8i
Serial No       : SV00601472
FW Package Build: 12.12.0-0111

                    Mfg. Data
                ================
Mfg. Date       : 02/02/10
Rework Date     : 00/00/00
Revision No     : 
Battery FRU     : N/A

                Image Versions in Flash:
                ================
FW Version         : 2.130.353-1663
BIOS Version       : 3.24.00_4.12.05.00_0x05160000
Preboot CLI Version: 04.04-020:#%00009
WebBIOS Version    : 6.0-49-e_45-Rel
NVDATA Version     : 2.09.03-0032
Boot Block Version : 2.02.00.00-0000
BOOT Version       : 09.250.01.219

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Vendor Id       : 1000
Device Id       : 0079
SubVendorId     : 1014
SubDeviceId     : 03b2

Host Interface  : PCIE

Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        4433221104000000 
1        4433221105000000 
2        4433221107000000 
3        4433221106000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 500605b001e4bb80
BBU              : Present
Alarm            : Present
NVRAM            : Present
Serial Debugger  : Present
Memory           : Present
Flash            : Present
Memory Size      : 512MB
TPM              : Absent
On board Expander: Absent

                Settings
                ================
Current Time                     : 11:18:23 7/31, 2012
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 2s
Physical Drive Coercion Mode     : Disabled
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Enabled
Ecc Bucket Size                  : 15
Ecc Bucket Leak Rate             : 1440 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Enabled
Maintain PD Fail History         : Enabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No

                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID6, RAID10, RAID50, RAID60, PRL 11, PRL 11 with spanning, SRL 3 supported
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed
Mix of SAS/SATA of HDD type in VD Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 128 
Max Number of VDs        : 64 
Max Parallel Commands    : 1008 
Max SGE Count            : 80 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 42 
Min Stripe Size          : 8 KB
Max Stripe Size          : 1.0 MB
Max Configurable SSC Size: 0 GB
Current Size of SSC      : 0 GB

                Device Present
                ================
Virtual Drives    : 1 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 5 
  Disks           : 4 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : Yes
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : Yes
Snapshot Enabled                : No
Support the OCE without adding drives : Yes

                Supported VD Operations
                ================
Read Policy          : Yes
Write Policy         : Yes
IO Policy            : Yes
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : No

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Disable Copyback                        : No
Enable JBOD                             : No
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : Yes
Enable SSD Patrol Read                  : No
PR Correct Unconfigured Areas           : Yes
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Stripe Size                      : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WB
Read Policy                      : Adaptive
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : Yes
Coercion Mode                    : None
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : No
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : Yes
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 16 
Disable Ctrl-R                   : Yes
Enable Web BIOS                  : Yes
Direct PD Mapping                : No
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : Yes
Maintain PD Fail History         : Yes
Disable Puncturing               : No
Zero Based Enclosure Enumeration : No
PreBoot CLI Enabled              : Yes
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : Yes
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : No
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : No
Max LD per array                 : 16
Power Saving option              : Not Defined
Default spin down time in minutes: 30 
Enable JBOD                      : No

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
ERROR: Failed to open file 2118ir.rom.

Exit Code: 0x01
ERROR: The image file is invalid and could not be flashed to the controller!!!

Exit Code: 0x01

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
ERROR: Failed to Validate The Image File 2118ir.bin. Stop!!!

Exit Code: 0x11
ERROR: Failed to Validate The Image File 2118it.bin. Stop!!!

Exit Code: 0x11
Adapter 0: LSI MegaRAID SAS 9260-8i
Vendor ID: 0x1000, Device ID: 0x0079

ERROR: The image file is invalid and could not be flashed to the controller!!!

Exit Code: 0x11
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01
Adapter 0: LSI MegaRAID SAS 9260-8i
Vendor ID: 0x1000, Device ID: 0x0079

ERROR: The image file is invalid and could not be flashed to the controller!!!

Exit Code: 0x11
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01

Controller Count: 1.

Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01
ERROR: Failed to Validate The Image File mptsas2.rom. Stop!!!

Exit Code: 0x11
ERROR: Failed to open file 2118ir.rom.
ERROR: Failed to Validate The Image File 2118ir.rom. Stop!!!

Exit Code: 0x11
ERROR: Failed to Validate The Image File 2118ir.bin. Stop!!!

Exit Code: 0x11
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

Exit Code: 0x00
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01

 Adapter #0: SubOemId is 0

Exit Code: 0x00
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01

Controller Count: 1.

Exit Code: 0x01
Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : LSI MegaRAID SAS 9260-8i
Serial No       : SV00601472
FW Package Build: 12.12.0-0111

                    Mfg. Data
                ================
Mfg. Date       : 02/02/10
Rework Date     : 00/00/00
Revision No     : 
Battery FRU     : N/A

                Image Versions in Flash:
                ================
FW Version         : 2.130.353-1663
BIOS Version       : 3.24.00_4.12.05.00_0x05160000
Preboot CLI Version: 04.04-020:#%00009
WebBIOS Version    : 6.0-49-e_45-Rel
NVDATA Version     : 2.09.03-0032
Boot Block Version : 2.02.00.00-0000
BOOT Version       : 09.250.01.219

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Vendor Id       : 1000
Device Id       : 0079
SubVendorId     : 1014
SubDeviceId     : 03b2

Host Interface  : PCIE

Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        0000000000000000 
1        0000000000000000 
2        0000000000000000 
3        0000000000000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 500605b001e4bb80
BBU              : Present
Alarm            : Present
NVRAM            : Present
Serial Debugger  : Present
Memory           : Present
Flash            : Present
Memory Size      : 512MB
TPM              : Absent
On board Expander: Absent

                Settings
                ================
Current Time                     : 12:23:6 8/4, 2012
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 2s
Physical Drive Coercion Mode     : Disabled
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Enabled
Ecc Bucket Size                  : 15
Ecc Bucket Leak Rate             : 1440 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Enabled
Maintain PD Fail History         : Enabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No

                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID6, RAID10, RAID50, RAID60, PRL 11, PRL 11 with spanning, SRL 3 supported
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed
Mix of SAS/SATA of HDD type in VD Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 128 
Max Number of VDs        : 64 
Max Parallel Commands    : 1008 
Max SGE Count            : 80 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 42 
Min Stripe Size          : 8 KB
Max Stripe Size          : 1.0 MB
Max Configurable SSC Size: 0 GB
Current Size of SSC      : 0 GB

                Device Present
                ================
Virtual Drives    : 0 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 1 
  Disks           : 0 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : Yes
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : Yes
Snapshot Enabled                : No
Support the OCE without adding drives : Yes

                Supported VD Operations
                ================
Read Policy          : Yes
Write Policy         : Yes
IO Policy            : Yes
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : No

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Disable Copyback                        : No
Enable JBOD                             : No
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : Yes
Enable SSD Patrol Read                  : No
PR Correct Unconfigured Areas           : Yes
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Stripe Size                      : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WB
Read Policy                      : Adaptive
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : Yes
Coercion Mode                    : None
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : No
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : Yes
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 16 
Disable Ctrl-R                   : Yes
Enable Web BIOS                  : Yes
Direct PD Mapping                : No
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : Yes
Maintain PD Fail History         : Yes
Disable Puncturing               : No
Zero Based Enclosure Enumeration : No
PreBoot CLI Enabled              : Yes
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : Yes
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : No
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : No
Max LD per array                 : 16
Power Saving option              : Not Defined
Default spin down time in minutes: 30 
Enable JBOD                      : No

Exit Code: 0x00

Controller Count: 1.

Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
ERROR: The image file is invalid and could not be flashed to the controller!!!

Exit Code: 0x01
Controller 0 (bus 4, device 0 ):
Vendor ID: 0x1000, Device ID: 0x0079


Erasing block at address f6360000
Erasing block at address f6380000
Erasing block at address f63a0000

Programming address f6360000
Programming address f6364000
Programming address f6368000
Programming address f636c000
Programming address f6370000
Programming address f6374000
Programming address f6378000
Programming address f637c000
Programming address f6380000
Programming address f6384000
Programming address f6388000
Programming address f638c000
Programming address f6390000
Programming address f6394000
Programming address f6398000
Programming address f639c000
Programming address f63a0000
Programming address f63a4000
Programming address f63a8000
Programming address f63ac000
Programming address f63b0000
Programming address f63b4000
Programming address f63b8000
Programming address f63bc000

Verifying address f6360000
Verifying address f6361000
Verifying address f6362000
Verifying address f6363000
Verifying address f6364000
Verifying address f6365000
Verifying address f6366000
Verifying address f6367000
Verifying address f6368000
Verifying address f6369000
Verifying address f636a000
Verifying address f636b000
Verifying address f636c000
Verifying address f636d000
Verifying address f636e000
Verifying address f636f000
Verifying address f6370000
Verifying address f6371000
Verifying address f6372000
Verifying address f6373000
Verifying address f6374000
Verifying address f6375000
Verifying address f6376000
Verifying address f6377000
Verifying address f6378000
Verifying address f6379000
Verifying address f637a000
Verifying address f637b000
Verifying address f637c000
Verifying address f637d000
Verifying address f637e000
Verifying address f637f000
Verifying address f6380000
Verifying address f6381000
Verifying address f6382000
Verifying address f6383000
Verifying address f6384000
Verifying address f6385000
Verifying address f6386000
Verifying address f6387000
Verifying address f6388000
Verifying address f6389000
Verifying address f638a000
Verifying address f638b000
Verifying address f638c000
Verifying address f638d000
Verifying address f638e000
Verifying address f638f000
Verifying address f6390000
Verifying address f6391000
Verifying address f6392000
Verifying address f6393000
Verifying address f6394000
Verifying address f6395000
Verifying address f6396000
Verifying address f6397000
Verifying address f6398000
Verifying address f6399000
Verifying address f639a000
Verifying address f639b000
Verifying address f639c000
Verifying address f639d000
Verifying address f639e000
Verifying address f639f000
Verifying address f63a0000
Verifying address f63a1000
Verifying address f63a2000
Verifying address f63a3000
Verifying address f63a4000
Verifying address f63a5000
Verifying address f63a6000
Verifying address f63a7000
Verifying address f63a8000
Verifying address f63a9000
Verifying address f63aa000
Verifying address f63ab000
Verifying address f63ac000
Verifying address f63ad000
Verifying address f63ae000
Verifying address f63af000
Verifying address f63b0000
Verifying address f63b1000
Verifying address f63b2000
Verifying address f63b3000
Verifying address f63b4000
Verifying address f63b5000
Verifying address f63b6000
Verifying address f63b7000
Verifying address f63b8000
Verifying address f63b9000
Verifying address f63ba000
Verifying address f63bb000
Verifying address f63bc000
Verifying address f63bd000
Verifying address f63be000
Verifying address f63bf000

Erasing block at address f63c0000
Erasing block at address f63e0000
Erasing block at address f6400000
Erasing block at address f6420000

Programming address f63c0000
Programming address f63c4000
Programming address f63c8000
Programming address f63cc000
Programming address f63d0000
Programming address f63d4000
Programming address f63d8000
Programming address f63dc000
Programming address f63e0000
Programming address f63e4000
Programming address f63e8000
Programming address f63ec000
Programming address f63f0000
Programming address f63f4000
Programming address f63f8000
Programming address f63fc000
Programming address f6400000
Programming address f6404000
Programming address f6408000
Programming address f640c000
Programming address f6410000
Programming address f6414000
Programming address f6418000
Programming address f641c000
Programming address f6420000
Programming address f6424000
Programming address f6428000
Programming address f642c000
Programming address f6430000
Programming address f6434000
Programming address f6438000
Programming address f643c000

Verifying address f63c0000
Verifying address f63c1000
Verifying address f63c2000
Verifying address f63c3000
Verifying address f63c4000
Verifying address f63c5000
Verifying address f63c6000
Verifying address f63c7000
Verifying address f63c8000
Verifying address f63c9000
Verifying address f63ca000
Verifying address f63cb000
Verifying address f63cc000
Verifying address f63cd000
Verifying address f63ce000
Verifying address f63cf000
Verifying address f63d0000
Verifying address f63d1000
Verifying address f63d2000
Verifying address f63d3000
Verifying address f63d4000
Verifying address f63d5000
Verifying address f63d6000
Verifying address f63d7000
Verifying address f63d8000
Verifying address f63d9000
Verifying address f63da000
Verifying address f63db000
Verifying address f63dc000
Verifying address f63dd000
Verifying address f63de000
Verifying address f63df000
Verifying address f63e0000
Verifying address f63e1000
Verifying address f63e2000
Verifying address f63e3000
Verifying address f63e4000
Verifying address f63e5000
Verifying address f63e6000
Verifying address f63e7000
Verifying address f63e8000
Verifying address f63e9000
Verifying address f63ea000
Verifying address f63eb000
Verifying address f63ec000
Verifying address f63ed000
Verifying address f63ee000
Verifying address f63ef000
Verifying address f63f0000
Verifying address f63f1000
Verifying address f63f2000
Verifying address f63f3000
Verifying address f63f4000
Verifying address f63f5000
Verifying address f63f6000
Verifying address f63f7000
Verifying address f63f8000
Verifying address f63f9000
Verifying address f63fa000
Verifying address f63fb000
Verifying address f63fc000
Verifying address f63fd000
Verifying address f63fe000
Verifying address f63ff000
Verifying address f6400000
Verifying address f6401000
Verifying address f6402000
Verifying address f6403000
Verifying address f6404000
Verifying address f6405000
Verifying address f6406000
Verifying address f6407000
Verifying address f6408000
Verifying address f6409000
Verifying address f640a000
Verifying address f640b000
Verifying address f640c000
Verifying address f640d000
Verifying address f640e000
Verifying address f640f000
Verifying address f6410000
Verifying address f6411000
Verifying address f6412000
Verifying address f6413000
Verifying address f6414000
Verifying address f6415000
Verifying address f6416000
Verifying address f6417000
Verifying address f6418000
Verifying address f6419000
Verifying address f641a000
Verifying address f641b000
Verifying address f641c000
Verifying address f641d000
Verifying address f641e000
Verifying address f641f000
Verifying address f6420000
Verifying address f6421000
Verifying address f6422000
Verifying address f6423000
Verifying address f6424000
Verifying address f6425000
Verifying address f6426000
Verifying address f6427000
Verifying address f6428000
Verifying address f6429000
Verifying address f642a000
Verifying address f642b000
Verifying address f642c000
Verifying address f642d000
Verifying address f642e000
Verifying address f642f000
Verifying address f6430000
Verifying address f6431000
Verifying address f6432000
Verifying address f6433000
Verifying address f6434000
Verifying address f6435000
Verifying address f6436000
Verifying address f6437000
Verifying address f6438000
Verifying address f6439000
Verifying address f643a000
Verifying address f643b000
Verifying address f643c000
Verifying address f643d000
Verifying address f643e000
Verifying address f643f000

Erasing block at address f6300000
Erasing block at address f6320000
Erasing block at address f6340000
Erasing block at address f6360000
Erasing block at address f6380000
Erasing block at address f63a0000
Erasing block at address f63c0000
Erasing block at address f63e0000
Erasing block at address f6400000
Erasing block at address f6420000
Erasing block at address f6440000
Erasing block at address f6460000
Erasing block at address f6480000
Erasing block at address f64a0000
Erasing block at address f64c0000
Erasing block at address f64e0000

Programming address f6300000
Programming address f6304000
Programming address f6308000
Programming address f630c000
Programming address f6310000
Programming address f6314000
Programming address f6318000
Programming address f631c000
Programming address f6320000
Programming address f6324000
Programming address f6328000
Programming address f632c000
Programming address f6330000
Programming address f6334000
Programming address f6338000
Programming address f633c000
Programming address f6340000
Programming address f6344000
Programming address f6348000
Programming address f634c000
Programming address f6350000
Programming address f6354000
Programming address f6358000
Programming address f635c000
Programming address f6360000
Programming address f6364000
Programming address f6368000
Programming address f636c000
Programming address f6370000
Programming address f6374000
Programming address f6378000
Programming address f637c000
Programming address f6380000
Programming address f6384000
Programming address f6388000
Programming address f638c000
Programming address f6390000
Programming address f6394000
Programming address f6398000
Programming address f639c000
Programming address f63a0000
Programming address f63a4000
Programming address f63a8000
Programming address f63ac000
Programming address f63b0000
Programming address f63b4000
Programming address f63b8000
Programming address f63bc000
Programming address f63c0000
Programming address f63c4000
Programming address f63c8000
Programming address f63cc000
Programming address f63d0000
Programming address f63d4000
Programming address f63d8000
Programming address f63dc000
Programming address f63e0000
Programming address f63e4000
Programming address f63e8000
Programming address f63ec000
Programming address f63f0000
Programming address f63f4000
Programming address f63f8000
Programming address f63fc000
Programming address f6400000
Programming address f6404000
Programming address f6408000
Programming address f640c000
Programming address f6410000
Programming address f6414000
Programming address f6418000
Programming address f641c000
Programming address f6420000
Programming address f6424000
Programming address f6428000
Programming address f642c000
Programming address f6430000
Programming address f6434000
Programming address f6438000
Programming address f643c000
Programming address f6440000
Programming address f6444000
Programming address f6448000
Programming address f644c000
Programming address f6450000
Programming address f6454000
Programming address f6458000
Programming address f645c000
Programming address f6460000
Programming address f6464000
Programming address f6468000
Programming address f646c000
Programming address f6470000
Programming address f6474000
Programming address f6478000
Programming address f647c000
Programming address f6480000
Programming address f6484000
Programming address f6488000
Programming address f648c000
Programming address f6490000
Programming address f6494000
Programming address f6498000
Programming address f649c000
Programming address f64a0000
Programming address f64a4000
Programming address f64a8000
Programming address f64ac000
Programming address f64b0000
Programming address f64b4000
Programming address f64b8000
Programming address f64bc000
Programming address f64c0000
Programming address f64c4000
Programming address f64c8000
Programming address f64cc000
Programming address f64d0000
Programming address f64d4000
Programming address f64d8000
Programming address f64dc000
Programming address f64e0000
Programming address f64e4000
Programming address f64e8000
Programming address f64ec000
Programming address f64f0000
Programming address f64f4000
Programming address f64f8000
Programming address f64fc000

Verifying address f6300000
Verifying address f6301000
Verifying address f6302000
Verifying address f6303000
Verifying address f6304000
Verifying address f6305000
Verifying address f6306000
Verifying address f6307000
Verifying address f6308000
Verifying address f6309000
Verifying address f630a000
Verifying address f630b000
Verifying address f630c000
Verifying address f630d000
Verifying address f630e000
Verifying address f630f000
Verifying address f6310000
Verifying address f6311000
Verifying address f6312000
Verifying address f6313000
Verifying address f6314000
Verifying address f6315000
Verifying address f6316000
Verifying address f6317000
Verifying address f6318000
Verifying address f6319000
Verifying address f631a000
Verifying address f631b000
Verifying address f631c000
Verifying address f631d000
Verifying address f631e000
Verifying address f631f000
Verifying address f6320000
Verifying address f6321000
Verifying address f6322000
Verifying address f6323000
Verifying address f6324000
Verifying address f6325000
Verifying address f6326000
Verifying address f6327000
Verifying address f6328000
Verifying address f6329000
Verifying address f632a000
Verifying address f632b000
Verifying address f632c000
Verifying address f632d000
Verifying address f632e000
Verifying address f632f000
Verifying address f6330000
Verifying address f6331000
Verifying address f6332000
Verifying address f6333000
Verifying address f6334000
Verifying address f6335000
Verifying address f6336000
Verifying address f6337000
Verifying address f6338000
Verifying address f6339000
Verifying address f633a000
Verifying address f633b000
Verifying address f633c000
Verifying address f633d000
Verifying address f633e000
Verifying address f633f000
Verifying address f6340000
Verifying address f6341000
Verifying address f6342000
Verifying address f6343000
Verifying address f6344000
Verifying address f6345000
Verifying address f6346000
Verifying address f6347000
Verifying address f6348000
Verifying address f6349000
Verifying address f634a000
Verifying address f634b000
Verifying address f634c000
Verifying address f634d000
Verifying address f634e000
Verifying address f634f000
Verifying address f6350000
Verifying address f6351000
Verifying address f6352000
Verifying address f6353000
Verifying address f6354000
Verifying address f6355000
Verifying address f6356000
Verifying address f6357000
Verifying address f6358000
Verifying address f6359000
Verifying address f635a000
Verifying address f635b000
Verifying address f635c000
Verifying address f635d000
Verifying address f635e000
Verifying address f635f000
Verifying address f6360000
Verifying address f6361000
Verifying address f6362000
Verifying address f6363000
Verifying address f6364000
Verifying address f6365000
Verifying address f6366000
Verifying address f6367000
Verifying address f6368000
Verifying address f6369000
Verifying address f636a000
Verifying address f636b000
Verifying address f636c000
Verifying address f636d000
Verifying address f636e000
Verifying address f636f000
Verifying address f6370000
Verifying address f6371000
Verifying address f6372000
Verifying address f6373000
Verifying address f6374000
Verifying address f6375000
Verifying address f6376000
Verifying address f6377000
Verifying address f6378000
Verifying address f6379000
Verifying address f637a000
Verifying address f637b000
Verifying address f637c000
Verifying address f637d000
Verifying address f637e000
Verifying address f637f000
Verifying address f6380000
Verifying address f6381000
Verifying address f6382000
Verifying address f6383000
Verifying address f6384000
Verifying address f6385000
Verifying address f6386000
Verifying address f6387000
Verifying address f6388000
Verifying address f6389000
Verifying address f638a000
Verifying address f638b000
Verifying address f638c000
Verifying address f638d000
Verifying address f638e000
Verifying address f638f000
Verifying address f6390000
Verifying address f6391000
Verifying address f6392000
Verifying address f6393000
Verifying address f6394000
Verifying address f6395000
Verifying address f6396000
Verifying address f6397000
Verifying address f6398000
Verifying address f6399000
Verifying address f639a000
Verifying address f639b000
Verifying address f639c000
Verifying address f639d000
Verifying address f639e000
Verifying address f639f000
Verifying address f63a0000
Verifying address f63a1000
Verifying address f63a2000
Verifying address f63a3000
Verifying address f63a4000
Verifying address f63a5000
Verifying address f63a6000
Verifying address f63a7000
Verifying address f63a8000
Verifying address f63a9000
Verifying address f63aa000
Verifying address f63ab000
Verifying address f63ac000
Verifying address f63ad000
Verifying address f63ae000
Verifying address f63af000
Verifying address f63b0000
Verifying address f63b1000
Verifying address f63b2000
Verifying address f63b3000
Verifying address f63b4000
Verifying address f63b5000
Verifying address f63b6000
Verifying address f63b7000
Verifying address f63b8000
Verifying address f63b9000
Verifying address f63ba000
Verifying address f63bb000
Verifying address f63bc000
Verifying address f63bd000
Verifying address f63be000
Verifying address f63bf000
Verifying address f63c0000
Verifying address f63c1000
Verifying address f63c2000
Verifying address f63c3000
Verifying address f63c4000
Verifying address f63c5000
Verifying address f63c6000
Verifying address f63c7000
Verifying address f63c8000
Verifying address f63c9000
Verifying address f63ca000
Verifying address f63cb000
Verifying address f63cc000
Verifying address f63cd000
Verifying address f63ce000
Verifying address f63cf000
Verifying address f63d0000
Verifying address f63d1000
Verifying address f63d2000
Verifying address f63d3000
Verifying address f63d4000
Verifying address f63d5000
Verifying address f63d6000
Verifying address f63d7000
Verifying address f63d8000
Verifying address f63d9000
Verifying address f63da000
Verifying address f63db000
Verifying address f63dc000
Verifying address f63dd000
Verifying address f63de000
Verifying address f63df000
Verifying address f63e0000
Verifying address f63e1000
Verifying address f63e2000
Verifying address f63e3000
Verifying address f63e4000
Verifying address f63e5000
Verifying address f63e6000
Verifying address f63e7000
Verifying address f63e8000
Verifying address f63e9000
Verifying address f63ea000
Verifying address f63eb000
Verifying address f63ec000
Verifying address f63ed000
Verifying address f63ee000
Verifying address f63ef000
Verifying address f63f0000
Verifying address f63f1000
Verifying address f63f2000
Verifying address f63f3000
Verifying address f63f4000
Verifying address f63f5000
Verifying address f63f6000
Verifying address f63f7000
Verifying address f63f8000
Verifying address f63f9000
Verifying address f63fa000
Verifying address f63fb000
Verifying address f63fc000
Verifying address f63fd000
Verifying address f63fe000
Verifying address f63ff000
Verifying address f6400000
Verifying address f6401000
Verifying address f6402000
Verifying address f6403000
Verifying address f6404000
Verifying address f6405000
Verifying address f6406000
Verifying address f6407000
Verifying address f6408000
Verifying address f6409000
Verifying address f640a000
Verifying address f640b000
Verifying address f640c000
Verifying address f640d000
Verifying address f640e000
Verifying address f640f000
Verifying address f6410000
Verifying address f6411000
Verifying address f6412000
Verifying address f6413000
Verifying address f6414000
Verifying address f6415000
Verifying address f6416000
Verifying address f6417000
Verifying address f6418000
Verifying address f6419000
Verifying address f641a000
Verifying address f641b000
Verifying address f641c000
Verifying address f641d000
Verifying address f641e000
Verifying address f641f000
Verifying address f6420000
Verifying address f6421000
Verifying address f6422000
Verifying address f6423000
Verifying address f6424000
Verifying address f6425000
Verifying address f6426000
Verifying address f6427000
Verifying address f6428000
Verifying address f6429000
Verifying address f642a000
Verifying address f642b000
Verifying address f642c000
Verifying address f642d000
Verifying address f642e000
Verifying address f642f000
Verifying address f6430000
Verifying address f6431000
Verifying address f6432000
Verifying address f6433000
Verifying address f6434000
Verifying address f6435000
Verifying address f6436000
Verifying address f6437000
Verifying address f6438000
Verifying address f6439000
Verifying address f643a000
Verifying address f643b000
Verifying address f643c000
Verifying address f643d000
Verifying address f643e000
Verifying address f643f000
Verifying address f6440000
Verifying address f6441000
Verifying address f6442000
Verifying address f6443000
Verifying address f6444000
Verifying address f6445000
Verifying address f6446000
Verifying address f6447000
Verifying address f6448000
Verifying address f6449000
Verifying address f644a000
Verifying address f644b000
Verifying address f644c000
Verifying address f644d000
Verifying address f644e000
Verifying address f644f000
Verifying address f6450000
Verifying address f6451000
Verifying address f6452000
Verifying address f6453000
Verifying address f6454000
Verifying address f6455000
Verifying address f6456000
Verifying address f6457000
Verifying address f6458000
Verifying address f6459000
Verifying address f645a000
Verifying address f645b000
Verifying address f645c000
Verifying address f645d000
Verifying address f645e000
Verifying address f645f000
Verifying address f6460000
Verifying address f6461000
Verifying address f6462000
Verifying address f6463000
Verifying address f6464000
Verifying address f6465000
Verifying address f6466000
Verifying address f6467000
Verifying address f6468000
Verifying address f6469000
Verifying address f646a000
Verifying address f646b000
Verifying address f646c000
Verifying address f646d000
Verifying address f646e000
Verifying address f646f000
Verifying address f6470000
Verifying address f6471000
Verifying address f6472000
Verifying address f6473000
Verifying address f6474000
Verifying address f6475000
Verifying address f6476000
Verifying address f6477000
Verifying address f6478000
Verifying address f6479000
Verifying address f647a000
Verifying address f647b000
Verifying address f647c000
Verifying address f647d000
Verifying address f647e000
Verifying address f647f000
Verifying address f6480000
Verifying address f6481000
Verifying address f6482000
Verifying address f6483000
Verifying address f6484000
Verifying address f6485000
Verifying address f6486000
Verifying address f6487000
Verifying address f6488000
Verifying address f6489000
Verifying address f648a000
Verifying address f648b000
Verifying address f648c000
Verifying address f648d000
Verifying address f648e000
Verifying address f648f000
Verifying address f6490000
Verifying address f6491000
Verifying address f6492000
Verifying address f6493000
Verifying address f6494000
Verifying address f6495000
Verifying address f6496000
Verifying address f6497000
Verifying address f6498000
Verifying address f6499000
Verifying address f649a000
Verifying address f649b000
Verifying address f649c000
Verifying address f649d000
Verifying address f649e000
Verifying address f649f000
Verifying address f64a0000
Verifying address f64a1000
Verifying address f64a2000
Verifying address f64a3000
Verifying address f64a4000
Verifying address f64a5000
Verifying address f64a6000
Verifying address f64a7000
Verifying address f64a8000
Verifying address f64a9000
Verifying address f64aa000
Verifying address f64ab000
Verifying address f64ac000
Verifying address f64ad000
Verifying address f64ae000
Verifying address f64af000
Verifying address f64b0000
Verifying address f64b1000
Verifying address f64b2000
Verifying address f64b3000
Verifying address f64b4000
Verifying address f64b5000
Verifying address f64b6000
Verifying address f64b7000
Verifying address f64b8000
Verifying address f64b9000
Verifying address f64ba000
Verifying address f64bb000
Verifying address f64bc000
Verifying address f64bd000
Verifying address f64be000
Verifying address f64bf000
Verifying address f64c0000
Verifying address f64c1000
Verifying address f64c2000
Verifying address f64c3000
Verifying address f64c4000
Verifying address f64c5000
Verifying address f64c6000
Verifying address f64c7000
Verifying address f64c8000
Verifying address f64c9000
Verifying address f64ca000
Verifying address f64cb000
Verifying address f64cc000
Verifying address f64cd000
Verifying address f64ce000
Verifying address f64cf000
Verifying address f64d0000
Verifying address f64d1000
Verifying address f64d2000
Verifying address f64d3000
Verifying address f64d4000
Verifying address f64d5000
Verifying address f64d6000
Verifying address f64d7000
Verifying address f64d8000
Verifying address f64d9000
Verifying address f64da000
Verifying address f64db000
Verifying address f64dc000
Verifying address f64dd000
Verifying address f64de000
Verifying address f64df000
Verifying address f64e0000
Verifying address f64e1000
Verifying address f64e2000
Verifying address f64e3000
Verifying address f64e4000
Verifying address f64e5000
Verifying address f64e6000
Verifying address f64e7000
Verifying address f64e8000
Verifying address f64e9000
Verifying address f64ea000
Verifying address f64eb000
Verifying address f64ec000
Verifying address f64ed000
Verifying address f64ee000
Verifying address f64ef000
Verifying address f64f0000
Verifying address f64f1000
Verifying address f64f2000
Verifying address f64f3000
Verifying address f64f4000
Verifying address f64f5000
Verifying address f64f6000
Verifying address f64f7000
Verifying address f64f8000
Verifying address f64f9000
Verifying address f64fa000
Verifying address f64fb000
Verifying address f64fc000
Verifying address f64fd000
Verifying address f64fe000
Verifying address f64ff000

Erasing block at address f6760000
Erasing block at address f6780000
Erasing block at address f67a0000
Erasing block at address f67c0000

Programming address f6760000
Programming address f6764000
Programming address f6768000
Programming address f676c000
Programming address f6770000
Programming address f6774000
Programming address f6778000
Programming address f677c000
Programming address f6780000
Programming address f6784000
Programming address f6788000
Programming address f678c000
Programming address f6790000
Programming address f6794000
Programming address f6798000
Programming address f679c000
Programming address f67a0000
Programming address f67a4000
Programming address f67a8000
Programming address f67ac000
Programming address f67b0000
Programming address f67b4000
Programming address f67b8000
Programming address f67bc000
Programming address f67c0000
Programming address f67c4000
Programming address f67c8000
Programming address f67cc000
Programming address f67d0000
Programming address f67d4000
Programming address f67d8000
Programming address f67dc000

Verifying address f6760000
Verifying address f6761000
Verifying address f6762000
Verifying address f6763000
Verifying address f6764000
Verifying address f6765000
Verifying address f6766000
Verifying address f6767000
Verifying address f6768000
Verifying address f6769000
Verifying address f676a000
Verifying address f676b000
Verifying address f676c000
Verifying address f676d000
Verifying address f676e000
Verifying address f676f000
Verifying address f6770000
Verifying address f6771000
Verifying address f6772000
Verifying address f6773000
Verifying address f6774000
Verifying address f6775000
Verifying address f6776000
Verifying address f6777000
Verifying address f6778000
Verifying address f6779000
Verifying address f677a000
Verifying address f677b000
Verifying address f677c000
Verifying address f677d000
Verifying address f677e000
Verifying address f677f000
Verifying address f6780000
Verifying address f6781000
Verifying address f6782000
Verifying address f6783000
Verifying address f6784000
Verifying address f6785000
Verifying address f6786000
Verifying address f6787000
Verifying address f6788000
Verifying address f6789000
Verifying address f678a000
Verifying address f678b000
Verifying address f678c000
Verifying address f678d000
Verifying address f678e000
Verifying address f678f000
Verifying address f6790000
Verifying address f6791000
Verifying address f6792000
Verifying address f6793000
Verifying address f6794000
Verifying address f6795000
Verifying address f6796000
Verifying address f6797000
Verifying address f6798000
Verifying address f6799000
Verifying address f679a000
Verifying address f679b000
Verifying address f679c000
Verifying address f679d000
Verifying address f679e000
Verifying address f679f000
Verifying address f67a0000
Verifying address f67a1000
Verifying address f67a2000
Verifying address f67a3000
Verifying address f67a4000
Verifying address f67a5000
Verifying address f67a6000
Verifying address f67a7000
Verifying address f67a8000
Verifying address f67a9000
Verifying address f67aa000
Verifying address f67ab000
Verifying address f67ac000
Verifying address f67ad000
Verifying address f67ae000
Verifying address f67af000
Verifying address f67b0000
Verifying address f67b1000
Verifying address f67b2000
Verifying address f67b3000
Verifying address f67b4000
Verifying address f67b5000
Verifying address f67b6000
Verifying address f67b7000
Verifying address f67b8000
Verifying address f67b9000
Verifying address f67ba000
Verifying address f67bb000
Verifying address f67bc000
Verifying address f67bd000
Verifying address f67be000
Verifying address f67bf000
Verifying address f67c0000
Verifying address f67c1000
Verifying address f67c2000
Verifying address f67c3000
Verifying address f67c4000
Verifying address f67c5000
Verifying address f67c6000
Verifying address f67c7000
Verifying address f67c8000
Verifying address f67c9000
Verifying address f67ca000
Verifying address f67cb000
Verifying address f67cc000
Verifying address f67cd000
Verifying address f67ce000
Verifying address f67cf000
Verifying address f67d0000
Verifying address f67d1000
Verifying address f67d2000
Verifying address f67d3000
Verifying address f67d4000
Verifying address f67d5000
Verifying address f67d6000
Verifying address f67d7000
Verifying address f67d8000
Verifying address f67d9000
Verifying address f67da000
Verifying address f67db000
Verifying address f67dc000
Verifying address f67dd000
Verifying address f67de000
Verifying address f67df000

Erasing block at address f67e0000
Erasing block at address f6800000
Erasing block at address f6820000
Erasing block at address f6840000

Programming address f67e0000
Programming address f67e4000
Programming address f67e8000
Programming address f67ec000
Programming address f67f0000
Programming address f67f4000
Programming address f67f8000
Programming address f67fc000
Programming address f6800000
Programming address f6804000
Programming address f6808000
Programming address f680c000
Programming address f6810000
Programming address f6814000
Programming address f6818000
Programming address f681c000
Programming address f6820000
Programming address f6824000
Programming address f6828000
Programming address f682c000
Programming address f6830000
Programming address f6834000
Programming address f6838000
Programming address f683c000
Programming address f6840000
Programming address f6844000
Programming address f6848000
Programming address f684c000
Programming address f6850000
Programming address f6854000
Programming address f6858000
Programming address f685c000

Verifying address f67e0000
Verifying address f67e1000
Verifying address f67e2000
Verifying address f67e3000
Verifying address f67e4000
Verifying address f67e5000
Verifying address f67e6000
Verifying address f67e7000
Verifying address f67e8000
Verifying address f67e9000
Verifying address f67ea000
Verifying address f67eb000
Verifying address f67ec000
Verifying address f67ed000
Verifying address f67ee000
Verifying address f67ef000
Verifying address f67f0000
Verifying address f67f1000
Verifying address f67f2000
Verifying address f67f3000
Verifying address f67f4000
Verifying address f67f5000
Verifying address f67f6000
Verifying address f67f7000
Verifying address f67f8000
Verifying address f67f9000
Verifying address f67fa000
Verifying address f67fb000
Verifying address f67fc000
Verifying address f67fd000
Verifying address f67fe000
Verifying address f67ff000
Verifying address f6800000
Verifying address f6801000
Verifying address f6802000
Verifying address f6803000
Verifying address f6804000
Verifying address f6805000
Verifying address f6806000
Verifying address f6807000
Verifying address f6808000
Verifying address f6809000
Verifying address f680a000
Verifying address f680b000
Verifying address f680c000
Verifying address f680d000
Verifying address f680e000
Verifying address f680f000
Verifying address f6810000
Verifying address f6811000
Verifying address f6812000
Verifying address f6813000
Verifying address f6814000
Verifying address f6815000
Verifying address f6816000
Verifying address f6817000
Verifying address f6818000
Verifying address f6819000
Verifying address f681a000
Verifying address f681b000
Verifying address f681c000
Verifying address f681d000
Verifying address f681e000
Verifying address f681f000
Verifying address f6820000
Verifying address f6821000
Verifying address f6822000
Verifying address f6823000
Verifying address f6824000
Verifying address f6825000
Verifying address f6826000
Verifying address f6827000
Verifying address f6828000
Verifying address f6829000
Verifying address f682a000
Verifying address f682b000
Verifying address f682c000
Verifying address f682d000
Verifying address f682e000
Verifying address f682f000
Verifying address f6830000
Verifying address f6831000
Verifying address f6832000
Verifying address f6833000
Verifying address f6834000
Verifying address f6835000
Verifying address f6836000
Verifying address f6837000
Verifying address f6838000
Verifying address f6839000
Verifying address f683a000
Verifying address f683b000
Verifying address f683c000
Verifying address f683d000
Verifying address f683e000
Verifying address f683f000
Verifying address f6840000
Verifying address f6841000
Verifying address f6842000
Verifying address f6843000
Verifying address f6844000
Verifying address f6845000
Verifying address f6846000
Verifying address f6847000
Verifying address f6848000
Verifying address f6849000
Verifying address f684a000
Verifying address f684b000
Verifying address f684c000
Verifying address f684d000
Verifying address f684e000
Verifying address f684f000
Verifying address f6850000
Verifying address f6851000
Verifying address f6852000
Verifying address f6853000
Verifying address f6854000
Verifying address f6855000
Verifying address f6856000
Verifying address f6857000
Verifying address f6858000
Verifying address f6859000
Verifying address f685a000
Verifying address f685b000
Verifying address f685c000
Verifying address f685d000
Verifying address f685e000
Verifying address f685f000

Erasing block at address f6860000
Erasing block at address f6880000

Programming address f6860000
Programming address f6864000
Programming address f6868000
Programming address f686c000
Programming address f6870000
Programming address f6874000
Programming address f6878000
Programming address f687c000
Programming address f6880000
Programming address f6884000
Programming address f6888000
Programming address f688c000
Programming address f6890000
Programming address f6894000
Programming address f6898000
Programming address f689c000

Verifying address f6860000
Verifying address f6861000
Verifying address f6862000
Verifying address f6863000
Verifying address f6864000
Verifying address f6865000
Verifying address f6866000
Verifying address f6867000
Verifying address f6868000
Verifying address f6869000
Verifying address f686a000
Verifying address f686b000
Verifying address f686c000
Verifying address f686d000
Verifying address f686e000
Verifying address f686f000
Verifying address f6870000
Verifying address f6871000
Verifying address f6872000
Verifying address f6873000
Verifying address f6874000
Verifying address f6875000
Verifying address f6876000
Verifying address f6877000
Verifying address f6878000
Verifying address f6879000
Verifying address f687a000
Verifying address f687b000
Verifying address f687c000
Verifying address f687d000
Verifying address f687e000
Verifying address f687f000
Verifying address f6880000
Verifying address f6881000
Verifying address f6882000
Verifying address f6883000
Verifying address f6884000
Verifying address f6885000
Verifying address f6886000
Verifying address f6887000
Verifying address f6888000
Verifying address f6889000
Verifying address f688a000
Verifying address f688b000
Verifying address f688c000
Verifying address f688d000
Verifying address f688e000
Verifying address f688f000
Verifying address f6890000
Verifying address f6891000
Verifying address f6892000
Verifying address f6893000
Verifying address f6894000
Verifying address f6895000
Verifying address f6896000
Verifying address f6897000
Verifying address f6898000
Verifying address f6899000
Verifying address f689a000
Verifying address f689b000
Verifying address f689c000
Verifying address f689d000
Verifying address f689e000
Verifying address f689f000

Erasing block at address f6ae0000

Programming address f6ae0000
Programming address f6ae4000
Programming address f6ae8000
Programming address f6aec000
Programming address f6af0000
Programming address f6af4000
Programming address f6af8000
Programming address f6afc000

Verifying address f6ae0000
Verifying address f6ae1000
Verifying address f6ae2000
Verifying address f6ae3000
Verifying address f6ae4000
Verifying address f6ae5000
Verifying address f6ae6000
Verifying address f6ae7000
Verifying address f6ae8000
Verifying address f6ae9000
Verifying address f6aea000
Verifying address f6aeb000
Verifying address f6aec000
Verifying address f6aed000
Verifying address f6aee000
Verifying address f6aef000
Verifying address f6af0000
Verifying address f6af1000
Verifying address f6af2000
Verifying address f6af3000
Verifying address f6af4000
Verifying address f6af5000
Verifying address f6af6000
Verifying address f6af7000
Verifying address f6af8000
Verifying address f6af9000
Verifying address f6afa000
Verifying address f6afb000
Verifying address f6afc000
Verifying address f6afd000
Verifying address f6afe000
Verifying address f6aff000
Controller ( bus 4, device 0 ) is flashed. 

1 Controller is flashed. Please reboot the system...


Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


        	AdpM0Flash 
        	----------

Syntax: MegaCli -AdpM0Flash -f filename

Description: 
        Flashes the firmware in Mode 0 with the ROM file listed on the command line. This option supports the Mode 0 flash functionality. For Mode 0 flash, the adapter number is not valid. 

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


        	AdpFwFlash
        	----------

Syntax: MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n]-aN| -a0,1,2|-aALL

Description: 
        Flashes the firmware with the ROM file specified at the command line.
        The possible parameters are:
        NoSigChk: option forces the application to flash the firmware even if the check word on the file does not match the required check word for the adapter. This option flashes the firmware only if the existing firmware version on the adapter is lower than the version on the ROM image.
        NoVerChk: also, the application flashes the adapter firmware without checking the version of the firmware image. The version check applies only to the firmware (APP.ROM) version.
        FwType: adapter firmware type. Give the value of Fw-type in number.  
        n: 0:- App or defaut, 1:- TMMC
        This command also supports the Mode 0 flash functionality. For Mode 0 flash, the adapter number is not valid. There are two possible methods:
        - Select which adapter to flash after the adapters are detected.
        - Flash the firmware on all present adapters.
        XML output data is generated by this option.

Convention:   
          -aN         N specifies the adapter number for the command.
          -a0,1,2     Specifies the command is for adapters 0, 1, and 2. More than one adapter can be selected.
          -aALL       Specifies the command is for all adapters.

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


        	AdpFwFlash
        	----------

Syntax: MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n]-aN| -a0,1,2|-aALL

Description: 
        Flashes the firmware with the ROM file specified at the command line.
        The possible parameters are:
        NoSigChk: option forces the application to flash the firmware even if the check word on the file does not match the required check word for the adapter. This option flashes the firmware only if the existing firmware version on the adapter is lower than the version on the ROM image.
        NoVerChk: also, the application flashes the adapter firmware without checking the version of the firmware image. The version check applies only to the firmware (APP.ROM) version.
        FwType: adapter firmware type. Give the value of Fw-type in number.  
        n: 0:- App or defaut, 1:- TMMC
        This command also supports the Mode 0 flash functionality. For Mode 0 flash, the adapter number is not valid. There are two possible methods:
        - Select which adapter to flash after the adapters are detected.
        - Flash the firmware on all present adapters.
        XML output data is generated by this option.

Convention:   
          -aN         N specifies the adapter number for the command.
          -a0,1,2     Specifies the command is for adapters 0, 1, and 2. More than one adapter can be selected.
          -aALL       Specifies the command is for all adapters.

Exit Code: 0x00
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01

    MegaCLI SAS RAID Management Tool  Ver 8.04.07 May 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.



NOTE: The following options may be given at the end of any command below: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

MegaCli -v 
MegaCli -help|-h|? 
MegaCli -adpCount 
MegaCli -AdpSetProp {CacheFlushInterval -val} | { RebuildRate -val} 
    | {PatrolReadRate -val} | {BgiRate -val} | {CCRate -val} 
    | {ReconRate -val} | {SpinupDriveCount -val} | {SpinupDelay -val} 
    | {CoercionMode -val} | {ClusterEnable -val} | {PredFailPollInterval -val} 
    | {BatWarnDsbl -val} | {EccBucketSize -val} | {EccBucketLeakRate -val} 
    | {AbortCCOnError -val} | AlarmEnbl | AlarmDsbl | AlarmSilence 
    | {SMARTCpyBkEnbl -val} | {SSDSMARTCpyBkEnbl -val} | NCQEnbl | NCQDsbl 
    | {MaintainPdFailHistoryEnbl -val} | {RstrHotSpareOnInsert -val} 
    | {DisableOCR -val} | {BootWithPinnedCache -val} | {enblPI -val} | {PreventPIImport -val} 
    | {EnblSpinDownUnConfigDrvs -val} -aN|-a0,1,2|-aALL 
    | AutoEnhancedImportEnbl | AutoEnhancedImportDsbl -aN|-a0,1,2|-aALL 
    | {ExposeEnclDevicesEnbl -val}|{UseDiskActivityforLocate -val} -aN|-a0,1,2|-aALL 
    | {DsblSpinDownHsp -val} -aN|-a0,1,2|-aALL 
    | {SpinDownTime -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDrvCnt -val} -aN|-a0,1,2|-aALL 
    | {SpinUpEncDelay -val} | { Perfmode -val} -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -AutoDetectBackPlaneDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Auto Detect of SGPIO and i2c SEP. 
             1=Disable Auto Detect of SGPIO. 
             2=Disable Auto Detect of i2c SEP. 
             3=Disable Auto Detect of SGPIO and i2c SEP. 
MegaCli -AdpSetProp -CopyBackDsbl -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Copyback. 
             1=Disable Copyback. 
MegaCli -AdpSetProp -EnableJBOD -val -aN|-a0,1,2|-aALL 
       val - 0=Disable JBOD mode. 
             1=Enable JBOD mode. 
MegaCli -AdpSetProp -DsblCacheBypass -val -aN|-a0,1,2|-aALL 
       val - 0=Enable Cache Bypass. 
             1=Disable Cache Bypass. 
MegaCli -AdpSetProp -LoadBalanceMode -val -aN|-a0,1,2|-aALL 
       val - 0=Auto Load balance mode. 
             1=Disable Load balance mode. 
MegaCli -AdpSetProp -UseFDEOnlyEncrypt -val -aN|-a0,1,2|-aALL 
       val - 0=FDE and controller encryption (if HW supports) is allowed. 
             1=Only support FDE encryption, disallow controller encryption. 
MegaCli -AdpSetProp -PrCorrectUncfgdAreas -val -aN|-a0,1,2|-aALL 
       val - 0= Correcting Media error during PR is disabled. 
             1=Correcting Media error during PR is allowed. 
MegaCli -AdpSetProp -DsblSpinDownHSP -val -aN|-a0,1,2|-aALL 
       val - 0= Spinning down the Hot Spare is enabled. 
             1=Spinning down the Hot Spare is disabled. 
MegaCli -AdpSetProp -DefaultLdPSPolicy -Automatic| -None | -Maximum| -MaximumWithoutCaching -aN|-a0,1,2|-aALL 
MegaCli -AdpSetProp -DisableLdPS -interval n1 -time n2 -aN|-a0,1,2|-aALL 
       where n1 is the number of hours beginning at time n2 
       where n2 is the number of minutes from 12:00am 
MegaCli -AdpSetProp -ENABLEEGHSP -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency GHSP. 
			 1= Enabled Emergency GHSP. 
MegaCli -AdpSetProp -ENABLEEUG -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency UG as Spare. 
			 1= Enabled Emergency UG as Spare. 
MegaCli -AdpSetProp -ENABLEESMARTER -val -aN|-a0,1,2|-aALL 
	   val - 0= Disabled Emergency Spare as Smarter. 
			 1= Enabled Emergency Spare as Smarter. 
MegaCli -AdpSetProp -DPMenable -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Drive Performance Monitoring . 
             1=Enable Drive Performance Monitoring. 
MegaCli -AdpSetProp -SupportSSDPatrolRead -val -aN|-a0,1,2|-aALL 
       val - 0=Disable Patrol read for SSD drives . 
             1=Enable Patrol read for SSD drives. 
MegaCli -AdpGetProp CacheFlushInterval | RebuildRate | PatrolReadRate 
    | BgiRate | CCRate | ReconRate | SpinupDriveCount | SpinupDelay 
    | CoercionMode | ClusterEnable | PredFailPollInterval | BatWarnDsbl 
    | EccBucketSize | EccBucketLeakRate | EccBucketCount | AbortCCOnError 
    | AlarmDsply | SMARTCpyBkEnbl | SSDSMARTCpyBkEnbl | NCQDsply 
    | MaintainPdFailHistoryEnbl | RstrHotSpareOnInsert 
    | EnblSpinDownUnConfigDrvs  | DisableOCR 
    | BootWithPinnedCache | enblPI  | PreventPIImport | AutoEnhancedImportDsply | AutoDetectBackPlaneDsbl 
    | CopyBackDsbl | LoadBalanceMode | UseFDEOnlyEncrypt | WBSupport | EnableJBOD 
    | DsblCacheBypass | ExposeEnclDevicesEnbl | DsblSpinDownHsp | SpinDownTime 
    | PrCorrectUncfgdAreas | UseDiskActivityforLocate | ENABLEEGHSP | ENABLEEUG 
    | ENABLEESMARTER | -DPMenable | Perfmode -aN|-a0,1,2|-aALL 
    | DsblSpinDownHSP -aN|-a0,1,2|-aALL 
    | DefaultLdPSPolicy | DisableLdPsInterval | DisableLdPsTime  
    | SpinUpEncDrvCnt | SpinUpEncDelay  -aN|-a0,1,2|-aALL 
MegaCli -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpGetTime -aN|-a0,1,2|-aALL  
MegaCli -AdpSetTime yyyymmdd hh:mm:ss -aN   
MegaCli -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaCli -AdpBIOS -Enbl |-Dsbl | -SOE | -BE | EnblAutoSelectBootLd | DsblAutoSelectBootLd | -Dsply -aN|-a0,1,2|-aALL 
MegaCli -AdpBootDrive {-Set {-Lx | -physdrv[E0:S0]}} | {-Unset {-Lx | -physdrv[E0:S0]}} |-Get -aN|-a0,1,2|-aALL 
MegaCli -AdpAutoRbld -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL
MegaCli -AdpCacheFlush -aN|-a0,1,2|-aALL
MegaCli -AdpPR -Dsbl|EnblAuto|EnblMan|Start|Suspend|Resume|Stop|Info 
         |{SetDelay Val}|{-SetStartTime yyyymmdd hh}|{maxConcurrentPD Val} -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -Dsbl|-Info|{-ModeConc | -ModeSeq [-ExcludeLD -LN|-L0,1,2]
   [-SetStartTime yyyymmdd hh ] [-SetDelay val ] } -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetStartTime yyyymmdd hh -aN|-a0,1,2|-aALL
MegaCli -AdpCcSched -SetDelay val  -aN|-a0,1,2|-aALL
MegaCli -FwTermLog -BBUoff|BBUoffTemp|BBUon|Dsply|Clear -aN|-a0,1,2|-aALL
MegaCli -AdpAlILog -aN|-a0,1,2|-aALL 
MegaCli -AdpDiag [val] -aN|-a0,1,2|-aALL
          val - Time in second.
MegaCli -AdpBatTest -aN|-a0,1,2|-aALL
MegaCli -PDList -aN|-a0,1,2|-aALL 
MegaCli -PDGetNum -aN|-a0,1,2|-aALL 
MegaCli -pdInfo -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDOnline  -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDOffline -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeGood -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -PDMakeJBOD -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDHSP {-Set [-Dedicated [-ArrayN|-Array0,1,2...]] [-EnclAffinity] [-nonRevertible]} 
     |-Rmv -PhysDrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PDRbld -Start|-Stop|-Suspend|-Resume|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PDClear -Start|-Stop|-ShowProg |-ProgDsply 
        -PhysDrv [E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL  
MegaCli -PdLocate {[-Start] | -stop } -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdMarkMissing -physdrv[E0:S0,E1:S1,...] -aN|-a0,1,2|-aALL 
MegaCli -PdGetMissing -aN|-a0,1,2|-aALL 
MegaCli -PdReplaceMissing -physdrv[E0:S0] -arrayA, -rowB -aN 
MegaCli -PdPrpRmv [-UnDo] -physdrv[E0:S0] -aN|-a0,1,2|-aALL  
MegaCli -EncInfo -aN|-a0,1,2|-aALL 
MegaCli -EncStatus -aN|-a0,1,2|-aALL 
MegaCli -PhyInfo -phyM -aN|-a0,1,2|-aALL  
MegaCli -PhySetLinkSpeed -phyM -speed -aN|-a0,1,2|-aALL
MegaCli -LDInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetProp  {-Name LdNamestring} | -RW|RO|Blocked|RemoveBlocked | WT|WB [-Immediate]|RA|NORA | DsblPI 
        | Cached|Direct | -EnDskCache|DisDskCache | CachedBadBBU|NoCachedBadBBU
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDSetPowerPolicy -Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching 
        -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDGetProp  -Cache | -Access | -Name | -DskCache | -PSPolicy | Consistency  -Lx|-L0,1,2|-LALL  
        -aN|-a0,1,2|-aALL 
MegaCli -getLdExpansionInfo -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LdExpansion -pN -dontExpandArray -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -Cachecade -assign|-remove -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL
MegaCli -LDInit {-Start [-full]}|-Abort|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDCC {-Start [-force]}|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL 
MegaCli -LDBI -Enbl|-Dsbl|-getSetting|-Abort|-Suspend|-Resume|-ShowProg|-ProgDsply -Lx|-L0,1,2|-LALL -aN|-a0,1,2|-aALL  
MegaCli -LDRecon {-Start -rX [{-Add | -Rmv} -Physdrv[E0:S0,...]]}|-ShowProg|-ProgDsply 
        -Lx -aN 
MegaCli -LdPdInfo -aN|-a0,1,2|-aALL 
MegaCli -LDGetNum -aN|-a0,1,2|-aALL 
MegaCli -LDBBMClr -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -GetBbtEntries -Lx|-L0,1,2|-Lall -aN|-a0,1,2|-aALL 
MegaCli -CfgLdAdd -rX[E0:S0,E1:S1,...] [WT|WB] [NORA|RA] [Direct|Cached]
        [CachedBadBBU|NoCachedBadBBU] [-szXXX [-szYYY ...]]
        [-strpszM] [-Hsp[E0:S0,...]] [-AfterLdX] [-Force]|[FDE|CtrlBased]  
        [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgCacheCadeAdd -Physdrv[E0:S0,...] {-Name LdNamestring} -aN|-a0,1,2|-aALL 
MegaCli -CfgEachDskRaid0 [WT|WB] [NORA|RA] [Direct|Cached] [-enblPI] 
        [CachedBadBBU|NoCachedBadBBU] [-strpszM]|[FDE|CtrlBased] [-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN|-a0,1,2|-aALL
MegaCli -CfgClr -aN|-a0,1,2|-aALL 
MegaCli -CfgDsply -aN|-a0,1,2|-aALL 
MegaCli -CfgLdDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgCacheCadeDel -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -CfgFreeSpaceinfo -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -r10 -Array0[E0:S0,E1:S1] -Array1[E0:S0,E1:S1] [-ArrayX[E0:S0,E1:S1] ...] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r50 -Array0[E0:S0,E1:S1,E2:S2,...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSpanAdd -r60 -Array0[E0:S0,E1:S1,E2:S2,E3,S3...] -Array1[E0:S0,E1:S1,E2:S2,...] 
        [-ArrayX[E0:S0,E1:S1,E2:S2,E3,S3...] ...] [WT|WB] [NORA|RA] [Direct|Cached] 
        [CachedBadBBU|NoCachedBadBBU][-strpszM][-szXXX[-szYYY ...]][-AfterLdX]| 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgAllFreeDrv -rX [-SATAOnly] [-SpanCount XXX] [WT|WB] [NORA|RA] 
        [Direct|Cached] [CachedBadBBU|NoCachedBadBBU] [-strpszM]
        [-HspCount XX [-HspType -Dedicated|-EnclAffinity|-nonRevertible]] | 
        [FDE|CtrlBased] 
		[-Default| -Automatic| -None| -Maximum| -MaximumWithoutCaching] [-enblPI] -aN 
MegaCli -CfgSave -f filename -aN   
MegaCli -CfgRestore -f filename -aN   
MegaCli -CfgForeign -Scan | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Dsply [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Preview [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Import [x] | [-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
MegaCli -CfgForeign -Clear [x]|[-SecurityKey sssssssssss] -aN|-a0,1,2|-aALL    
        x - index of foreign configurations. Optional. All by default. 
MegaCli -AdpEventLog -GetEventLogInfo -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetEvents {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceShutdown {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetSinceReboot {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -IncludeDeleted {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetLatest n {-info -warning -critical -fatal} {-f <fileName>} -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -GetCCIncon -f <fileName> -LX|-L0,2,5...|-LALL -aN|-a0,1,2|-aALL 
MegaCli -AdpEventLog -Clear -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuStatus -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuCapacityInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuDesignInfo -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -GetBbuProperties -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuLearn -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSleep -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -BbuMfgSeal -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -getBbumodes  -aN|-a0,1,2|-aALL  
MegaCli -AdpBbuCmd -SetBbuProperties -f <fileName> -aN|-a0,1,2|-aALL 
MegaCli -AdpBbuCmd -ScheduleLearn -Dsbl|-Info|[-STARTTIME DDD hh] -aN|-a0,1,2|-aALL 
MegaCli -AdpFacDefSet -aN 
MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n] -aN|-a0,1,2|-aALL  
MegaCli -AdpM0Flash -f filename  
MegaCli -AdpGetConnectorMode -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -AdpSetConnectorMode -Internal|-External|-Auto -ConnectorN|-Connector0,1|-ConnectorAll -aN|-a0,1,2|-aALL  
MegaCli -PhyErrorCounters -aN|-a0,1,2|-aALL  
MegaCli -DirectPdMapping -Enbl|-Dsbl|-Dsply -aN|-a0,1,2|-aALL  
MegaCli -ShowEnclList -aN|-a0,1,2|-aALL 
MegaCli -ShowVpd -Page N -Encl N -aN|-a0,1,2|-aALL 
MegaCli -EnclLocate -Start|-Stop -Encl N -aN|-a0,1,2|-aALL  
MegaCli -PdFwDownload [offline][ForceActivate] {[-SataBridge] -PhysDrv[0:1] }|{-EncdevId[devId1]} -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -SetFacDefault -Encl N -Esm A|B -f <filename> -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Start -PhysDrv[E0:S0,E1:S1] -aN|-a0,1,2|-aALL 
MegaCli -PDCpyBk -Stop|-Suspend|-Resume|-ShowProg|-ProgDsply -PhysDrv[E0:S0] -aN|-a0,1,2|-aALL 
MegaCli -PDInstantSecureErase -PhysDrv[E0:S0,E1:S1,...] | [-Force] -aN|-a0,1,2|-aALL 
MegaCli -Version -Cli|-Ctrl|-Driver|-Pd -aN|-a0,1,2|-aALL 
MegaCli -CfgSpanAdd -rX -array0[E0:S1,E1:S1.....] array1[E0:S1,E1:S1.....] -szxxx -enblPI -aN|-a0,1,2|-aALL 
MegaCli -LDMakeSecure -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -DestroySecurityKey | [-Force] -aN 
MegaCli -CreateSecurityKey -SecurityKey sssssssssss | [-Passphrase sssssssssss] |[-KeyID kkkkkkkkkkk] -aN 
MegaCli -CreateSecurityKey useEKMS -aN 
MegaCli -ChangeSecurityKey -OldSecurityKey sssssssssss | -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey -SecurityKey sssssssssss| 
          [-Passphrase sssssssssss] | [-KeyID kkkkkkkkkkk] -aN
MegaCli -ChangeSecurityKey useEKMS -OldSecurityKey sssssssssss -aN
MegaCli -ChangeSecurityKey -useEKMS -aN
MegaCli -GetKeyID [-PhysDrv[E0:S0]] -aN 
MegaCli -SetKeyID -KeyID kkkkkkkkkkk -aN 
MegaCli -VerifySecurityKey -SecurityKey sssssssssss -aN 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -GetPreservedCacheList -aN|-a0,1,2|-aALL 
MegaCli -DiscardPreservedCache -Lx|-L0,1,2|-Lall -force -aN|-a0,1,2|-aALL 
MegaCli -AdpInfoCompare {-checkFw <string> | -checkID -hex | -checkBatt -val | -checkDimm -val} -aN|-a0,1,2|-aALL 
MegaCli -adpFwDump 
MegaCli -AdpNameRtn -aN|-a0,1,2|-aALL 

       sssssssssss  - It must be between eight and thirty-two 
                      characters and contain at least one number, 
                      one lowercase letter, one uppercase 
                      letter and one non-alphanumeric character.
       kkkkkkkkkkk -  Must be less than 256 characters. 
MegaCli -ShowSummary [-f filename] -aN
MegaCli -ELF -GetSafeId -aN|-a0,1,2|-aALL
MegaCli -ELF -ControllerFeatures -aN|-a0,1,2|-aALL
MegaCli -ELF -Applykey key <val> [Preview] -aN|-a0,1,2|-aALL
MegaCli -ELF -TransferToVault -aN|-a0,1,2|-aALL
MegaCli -ELF -DeactivateTrialKey -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostInfo -aN|-a0,1,2|-aALL
MegaCli -ELF -ReHostComplete -aN|-a0,1,2|-aALL
MegaCli -LDBreakMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -FullStrSeekTest -aN|-a0,1,2|-aALL 
MegaCli -LDViewMirror -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -LDJoinMirror -DataSrc <val>[-force] -Lx|-L0,1,2,...|-Lall -aN|-a0,1,2|-aALL 
MegaCli -SecureErase 
	Start[
		Simple|
		[Normal   [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]|
		[Thorough [ |ErasePattern ErasePatternA|ErasePattern ErasePatternA ErasePattern ErasePatternB]]]
	| Stop
	| ShowProg
	| ProgDsply 
	[-PhysDrv [E0:S0,E1:S1,...] | -Lx|-L0,1,2|-LALL] -aN|-a0,1,2|-aALL
MegaCli -Perfmon {-start -interval <val>} | {stop} | {-getresults -f <Filename>} -aN 
MegaCli -DpmStat -Dsply {lct | hist | ra | ext } [-physdrv[E0:S0]] -aN|-a0,1,2|-aALL  
MegaCli -DpmStat -Clear {lct | hist | ra | ext } -aN|-a0,1,2|-aALL  

    Note: The directly connected drives can be specified as [:S] 

    Wildcard '?' can be used to specify the enclosure ID for the drive in the 
      only enclosure without direct connected device or the direct connected 
      drives with no enclosure in the system.

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

      [-Silent] [-AppLogFile filename] [-NoLog] [-page [N]]
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

Controller Count: 1.

Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
User specified controller is not present.
Failed to get CpController object.

Exit Code: 0x01
Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : ServeRAID M5015 SAS/SATA Controller
Serial No       : SV00601472
FW Package Build: 12.12.0-0048

                    Mfg. Data
                ================
Mfg. Date       : 02/02/10
Rework Date     : 00/00/00
Revision No     : 
Battery FRU     : N/A

                Image Versions in Flash:
                ================
FW Version         : 2.120.63-1242
BIOS Version       : 3.22.00_4.11.05.00_0x05020000
Preboot CLI Version: 04.04-017:#%00008
WebBIOS Version    : 6.0-34-e_29-Rel
NVDATA Version     : 2.09.03-0013
Boot Block Version : 2.02.00.00-0000
BOOT Version       : 09.250.01.219

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Vendor Id       : 1000
Device Id       : 0079
SubVendorId     : 1014
SubDeviceId     : 03b2

Host Interface  : PCIE

Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        4433221102000000 
1        4433221103000000 
2        4433221104000000 
3        4433221105000000 
4        4433221106000000 
5        4433221107000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 500605b001e4bb80
BBU              : Present
Alarm            : Present
NVRAM            : Present
Serial Debugger  : Present
Memory           : Present
Flash            : Present
Memory Size      : 512MB
TPM              : Absent
On board Expander: Absent

                Settings
                ================
Current Time                     : 21:59:58 9/15, 2012
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 2s
Physical Drive Coercion Mode     : Disabled
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Enabled
Ecc Bucket Size                  : 15
Ecc Bucket Leak Rate             : 1440 Minutes
Restore HotSpare on Insertion    : Disabled
Expose Enclosure Devices         : Enabled
Maintain PD Fail History         : Enabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No

                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID6, RAID10, RAID50, RAID60, PRL 11, PRL 11 with spanning, SRL 3 supported
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed
Mix of SAS/SATA of HDD type in VD Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 128 
Max Number of VDs        : 64 
Max Parallel Commands    : 1008 
Max SGE Count            : 80 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 42 
Min Stripe Size          : 8 KB
Max Stripe Size          : 1.0 MB
Max Configurable SSC Size: 0 GB
Current Size of SSC      : 0 GB

                Device Present
                ================
Virtual Drives    : 6 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 7 
  Disks           : 6 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : Yes
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : Yes
Snapshot Enabled                : No
Support the OCE without adding drives : Yes

                Supported VD Operations
                ================
Read Policy          : Yes
Write Policy         : Yes
IO Policy            : Yes
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : No

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Disable Copyback                        : No
Enable JBOD                             : No
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : Yes
Enable SSD Patrol Read                  : No
PR Correct Unconfigured Areas           : Yes
Enable Spin Down of UnConfigured Drives : Yes
Disable Spin Down of hot spares         : No
Spin Down time                          : 30 
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Stripe Size                      : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WB
Read Policy                      : Adaptive
Cache When BBU Bad               : Disabled
Cached IO                        : No
SMART Mode                       : Mode 6
Alarm Disable                    : Yes
Coercion Mode                    : None
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : No
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : Yes
Allow SSD SAS/SATA Mix in VD     : No
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 16 
Disable Ctrl-R                   : Yes
Enable Web BIOS                  : Yes
Direct PD Mapping                : No
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : No
Expose Enclosure Devices         : Yes
Maintain PD Fail History         : Yes
Disable Puncturing               : No
Zero Based Enclosure Enumeration : No
PreBoot CLI Enabled              : Yes
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : Yes
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : No
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : No
Max LD per array                 : 16
Power Saving option              : Not Defined
Default spin down time in minutes: 30 
Enable JBOD                      : No

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
Clearing NVRAM on Adapter 0 Success!

Exit Code: 0x00
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
Adapter #0

==============================================================================
                    Versions
                ================
Product Name    : LSI MegaRAID SAS 9261-8i
Serial No       : SV12113715
FW Package Build: 12.12.0-0048

                    Mfg. Data
                ================
Mfg. Date       : 05/19/11
Rework Date     : 00/00/00
Revision No     : 24A
Battery FRU     : N/A

                Image Versions in Flash:
                ================
FW Version         : 2.120.63-1242
BIOS Version       : 3.22.00_4.11.05.00_0x05020000
Preboot CLI Version: 04.04-017:#%00008
WebBIOS Version    : 6.0-34-e_29-Rel
NVDATA Version     : 2.09.03-0013
Boot Block Version : 2.02.00.00-0000
BOOT Version       : 09.250.01.219

                Pending Images in Flash
                ================
None

                PCI Info
                ================
Vendor Id       : 1000
Device Id       : 0079
SubVendorId     : 1000
SubDeviceId     : 9263

Host Interface  : PCIE

Number of Frontend Port: 0 
Device Interface  : PCIE

Number of Backend Port: 8 
Port  :  Address
0        0000000000000000 
1        0000000000000000 
2        0000000000000000 
3        0000000000000000 
4        0000000000000000 
5        0000000000000000 
6        0000000000000000 
7        0000000000000000 

                HW Configuration
                ================
SAS Address      : 500605b0037a3ec0
BBU              : Present
Alarm            : Present
NVRAM            : Present
Serial Debugger  : Present
Memory           : Present
Flash            : Present
Memory Size      : 512MB
TPM              : Absent
On board Expander: Absent

                Settings
                ================
Current Time                     : 19:10:9 10/2, 2012
Predictive Fail Poll Interval    : 300sec
Interrupt Throttle Active Count  : 16
Interrupt Throttle Completion    : 50us
Rebuild Rate                     : 30%
PR Rate                          : 30%
BGI Rate                         : 30%
Check Consistency Rate           : 30%
Reconstruction Rate              : 30%
Cache Flush Interval             : 4s
Max Drives to Spinup at One Time : 4
Delay Among Spinup Groups        : 2s
Physical Drive Coercion Mode     : 1GB
Cluster Mode                     : Disabled
Alarm                            : Disabled
Auto Rebuild                     : Enabled
Battery Warning                  : Enabled
Ecc Bucket Size                  : 15
Ecc Bucket Leak Rate             : 1440 Minutes
Restore HotSpare on Insertion    : Enabled
Expose Enclosure Devices         : Enabled
Maintain PD Fail History         : Enabled
Host Request Reordering          : Enabled
Auto Detect BackPlane Enabled    : SGPIO/i2c SEP
Load Balance Mode                : Auto
Use FDE Only                     : Yes
Security Key Assigned            : No
Security Key Failed              : No
Security Key Not Backedup        : No
Any Offline VD Cache Preserved   : No
Allow Boot with Preserved Cache  : No
Disable Online Controller Reset  : No

                Capabilities
                ================
RAID Level Supported             : RAID0, RAID1, RAID5, RAID6, RAID10, RAID50, RAID60, PRL 11, PRL 11 with spanning, SRL 3 supported
Supported Drives                 : SAS, SATA

Allowed Mixing:

Mix in Enclosure Allowed
Mix of SAS/SATA of HDD type in VD Allowed
Mix of SAS/SATA of SSD type in VD Allowed

                Status
                ================
ECC Bucket Count                 : 0

                Limitations
                ================
Max Arms Per VD          : 32 
Max Spans Per VD         : 8 
Max Arrays               : 128 
Max Number of VDs        : 64 
Max Parallel Commands    : 1008 
Max SGE Count            : 60 
Max Data Transfer Size   : 8192 sectors 
Max Strips PerIO         : 42 
Min Stripe Size          : 8 KB
Max Stripe Size          : 1.0 MB
Max Configurable SSC Size: 512 GB
Current Size of SSC      : 0 GB

                Device Present
                ================
Virtual Drives    : 0 
  Degraded        : 0 
  Offline         : 0 
Physical Devices  : 1 
  Disks           : 0 
  Critical Disks  : 0 
  Failed Disks    : 0 

                Supported Adapter Operations
                ================
Rebuild Rate                    : Yes
CC Rate                         : Yes
BGI Rate                        : Yes
Reconstruct Rate                : Yes
Patrol Read Rate                : Yes
Alarm Control                   : Yes
Cluster Support                 : No
BBU                             : Yes
Spanning                        : Yes
Dedicated Hot Spare             : Yes
Revertible Hot Spares           : Yes
Foreign Config Import           : Yes
Self Diagnostic                 : Yes
Allow Mixed Redundancy on Array : No
Global Hot Spares               : Yes
Deny SCSI Passthrough           : No
Deny SMP Passthrough            : No
Deny STP Passthrough            : No
Support Security                : Yes
Snapshot Enabled                : Yes
Support the OCE without adding drives : Yes

                Supported VD Operations
                ================
Read Policy          : Yes
Write Policy         : Yes
IO Policy            : Yes
Access Policy        : Yes
Disk Cache Policy    : Yes
Reconstruction       : Yes
Deny Locate          : No
Deny CC              : No
Allow Ctrl Encryption: No
Enable LDBBM         : No

                Supported PD Operations
                ================
Force Online                            : Yes
Force Offline                           : Yes
Force Rebuild                           : Yes
Deny Force Failed                       : No
Deny Force Good/Bad                     : No
Deny Missing Replace                    : No
Deny Clear                              : No
Deny Locate                             : No
Disable Copyback                        : No
Enable JBOD                             : No
Enable Copyback on SMART                : No
Enable Copyback to SSD on SMART Error   : Yes
Enable SSD Patrol Read                  : No
PR Correct Unconfigured Areas           : Yes
Enable Spin Down of UnConfigured Drives : Yes
Disable Spin Down of hot spares         : No
Spin Down time                          : 30 
                Error Counters
                ================
Memory Correctable Errors   : 0 
Memory Uncorrectable Errors : 0 

                Cluster Information
                ================
Cluster Permitted     : No
Cluster Active        : No

                Default Settings
                ================
Phy Polarity                     : 0 
Phy PolaritySplit                : 0 
Background Rate                  : 30 
Stripe Size                      : 64kB
Flush Time                       : 4 seconds
Write Policy                     : WB
Read Policy                      : None
Cache When BBU Bad               : Disabled
Cached IO                        : Yes
SMART Mode                       : Mode 6
Alarm Disable                    : No
Coercion Mode                    : 1GB
ZCR Config                       : Unknown
Dirty LED Shows Drive Activity   : No
BIOS Continue on Error           : No
Spin Down Mode                   : None
Allowed Device Type              : SAS/SATA Mix
Allow Mix in Enclosure           : Yes
Allow HDD SAS/SATA Mix in VD     : Yes
Allow SSD SAS/SATA Mix in VD     : Yes
Allow HDD/SSD Mix in VD          : No
Allow SATA in Cluster            : No
Max Chained Enclosures           : 16 
Disable Ctrl-R                   : Yes
Enable Web BIOS                  : Yes
Direct PD Mapping                : No
BIOS Enumerate VDs               : Yes
Restore Hot Spare on Insertion   : Yes
Expose Enclosure Devices         : Yes
Maintain PD Fail History         : Yes
Disable Puncturing               : No
Zero Based Enclosure Enumeration : Yes
PreBoot CLI Enabled              : Yes
LED Show Drive Activity          : Yes
Cluster Disable                  : Yes
SAS Disable                      : No
Auto Detect BackPlane Enable     : SGPIO/i2c SEP
Use FDE Only                     : Yes
Enable Led Header                : Yes
Delay during POST                : 0 
EnableCrashDump                  : No
Disable Online Controller Reset  : No
EnableLDBBM                      : No
Un-Certified Hard Disk Drives    : Allow
Treat Single span R1E as R10     : No
Max LD per array                 : 16
Power Saving option              : Not Defined
Default spin down time in minutes: 30 
Enable JBOD                      : No

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.

Invalid input at or near token     ADPFW
Use -help to know command name

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


        	AdpFwFlash
        	----------

Syntax: MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n]-aN| -a0,1,2|-aALL

Description: 
        Flashes the firmware with the ROM file specified at the command line.
        The possible parameters are:
        NoSigChk: option forces the application to flash the firmware even if the check word on the file does not match the required check word for the adapter. This option flashes the firmware only if the existing firmware version on the adapter is lower than the version on the ROM image.
        NoVerChk: also, the application flashes the adapter firmware without checking the version of the firmware image. The version check applies only to the firmware (APP.ROM) version.
        FwType: adapter firmware type. Give the value of Fw-type in number.  
        n: 0:- App or defaut, 1:- TMMC
        This command also supports the Mode 0 flash functionality. For Mode 0 flash, the adapter number is not valid. There are two possible methods:
        - Select which adapter to flash after the adapters are detected.
        - Flash the firmware on all present adapters.
        XML output data is generated by this option.

Convention:   
          -aN         N specifies the adapter number for the command.
          -a0,1,2     Specifies the command is for adapters 0, 1, and 2. More than one adapter can be selected.
          -aALL       Specifies the command is for all adapters.

Exit Code: 0x00

    MegaCLI SAS RAID Management Tool  Ver 8.05.06 Aug 28, 2012

    (c)Copyright 2011, LSI Corporation, All Rights Reserved.


        	AdpFwFlash
        	----------

Syntax: MegaCli -AdpFwFlash -f filename [-NoSigChk] [-NoVerChk] [-FWTYPE n]-aN| -a0,1,2|-aALL

Description: 
        Flashes the firmware with the ROM file specified at the command line.
        The possible parameters are:
        NoSigChk: option forces the application to flash the firmware even if the check word on the file does not match the required check word for the adapter. This option flashes the firmware only if the existing firmware version on the adapter is lower than the version on the ROM image.
        NoVerChk: also, the application flashes the adapter firmware without checking the version of the firmware image. The version check applies only to the firmware (APP.ROM) version.
        FwType: adapter firmware type. Give the value of Fw-type in number.  
        n: 0:- App or defaut, 1:- TMMC
        This command also supports the Mode 0 flash functionality. For Mode 0 flash, the adapter number is not valid. There are two possible methods:
        - Select which adapter to flash after the adapters are detected.
        - Flash the firmware on all present adapters.
        XML output data is generated by this option.

Convention:   
          -aN         N specifies the adapter number for the command.
          -a0,1,2     Specifies the command is for adapters 0, 1, and 2. More than one adapter can be selected.
          -aALL       Specifies the command is for all adapters.

Exit Code: 0x00

Controller Count: 2.

Exit Code: 0x02
Fatal error - Command Tool invoked with wrong parameters
Exit Code: 0x01

    MegaOEM Ver 8.00.11 December 21, 2009

    (c)Copyright 2009, LSI Corporation, All Rights Reserved.


NOTE: The following options may be given at the end of any command below: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

MegaOEM -v 
MegaOEM -help|-h|? 
MegaOEM -adpCount 
MegaOEM -AdpAllInfo -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSASA xxxxxxxxxxxxxxxx -aN   
MegaOEM -AdpSettings Read | Write -f FileName -aN 
        -Read - reads INI file, forms MFC_DEFAULT structure and sends it to the FW. 
        -Write - reads MFC_DEFAULT structure and creates an INI file 
MegaOEM -AdpMfgSet -f fileName -aN  
MegaOEM -AdpSetVerify -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetVerifyRaw -f fileName -aN|-a0,1,2|-aALL  
MegaOEM -AdpSetSubOEMId XX -aN	
         XX - sub-OEM ID in Hexadecimal.
MegaOEM -AdpGetSubOEMId  -aN	
MegaOEM -adpUpdatePersistentPage -f filename - aN 
MegaOEM -AdpNVRAM {-Read | -Write -f FileName}|-Clear 
        [-StartOffset 0xXXXX ] [-EndOffset 0xXXXX] -aN 

      Note:[-aALL] option assumes that the parameters specified are valid 
       for all the Adapters. 

    The following options may be given at the end of any command above: 

    [-Silent] [-AppLogFile filename] [-NoLog] [-page[N]] 
                 [-] is optional. 
                  N - Number of lines per page. 

Exit Code: 0x00
